# Supplementary material



Figure S1. Spray-like jets for vent pipes with different diameter *d*: (a) *d* = 40 mm; (b) *d* = 60 mm.