Using submersible fluorescence sensors to track the removal of organic matter in decentralized wastewater treatment systems (DEWATS) in real time

**SUPPLEMENTARY MATERIAL**



Figure S1. Experimental ABR-AF-CW system with three treatment trains. Trains 1 and 2 have seven ABR chambers; Train 3 has four ABR chambers. Each chamber is equipped with hatch for sampling.